MCj03463170000[1]Safety Instruction

1. Users are required to read the operation manual completely and carefully before installation or operation.
2. The product should be installed and pre-operated by well-trained persons. All power supplies must be turned off during the installation work, remember not to operate with power on.
3. All the instruction marked with sign MCj03463170000[1] must be observed or executed; otherwise, bodily injuries might occur.
4. For perfect operation and safety, it is prohibited that using extension cable with multi-outlet for power connection.
5. When connecting the power cord, it must be determined that the operating voltage conforms to the rated voltage value specified in the product identification.
6. Don＇t operate in direct sun light，outdoors area and where the room temperature is over 45°C or below 0°C.
7. Please avoid operating near the heater at dew area or at the humidity below 10% or above 90%.
8. Don＇t operate in area with heavy dust, corrosive substance or volatile gas.
9. Avoid power cord being applied by heavy objects or excessive force, or over bend.
10. The earth wire of power cord must be connected to the system ground of the production plant by proper size of conductions and terminals. This connection should be fixed permanently.
11. All the moving portions must be prevented to be exposed by the parts provided.
12. Turing on the machine in the first time, operate the sewing machine at low speed and check the correct rotation direction.
13. Turn off the power before the following operation:

1. Connecting or disconnecting any connectors on the control box or motor.

2. Threading needle.

3. Raising the machine head.

4. Repairing or doing any mechanical adjustment.

5. Machines idling.

1. Repairs and high level maintenance work should only be carried out by electronic technicians with appropriate training.
2. All the spare parts for repair must be provided or approved by the manufacturer.
3. Don’t use any objects or force to hit or ram the product.

**Guarantee Time**

Warranty period of this product is 1 year dated from purchasing, or within 2 years from ex-factory date.

**Warranty Detail**

Any trouble found within warranty period under normal operation, it will be repaired free of charge. However, maintenance cost will be charged in the following cases even if within warranty period:

1. Inappropriate use, including: wrong connecting high voltage, wrong application, disassemble, repair, modification by incompetent personnel, or operation without the precaution, or operation out of its specification range, or inserting other objects or liquids into the product.

2. Damage by fire, Earth quake, lighting, wind, flood, salt corrosive, moisture, abnormal power voltage and any other damage cause by the natural disaster or by the inappropriate environments.

3. Dropping after purchasing or damage in transportation by customer himself or by customer’s shipping agency

\* We make our best effort to test and manufacture the product for assuring the quality. However, it is possible that this product can be damaged due to external magnetic interference and electronic static or noise or unstable power source more than expected; therefore the grounding system of operate area must guarantee the good earth and it’s also recommended to install a failsafe device (Such as residual current breaker).

**1 Key displays and operating instructions**

**1.1 Key description**

|  |  |  |
| --- | --- | --- |
| Name | key | Indicate |
| Stitch length setting |  | If click, increase or decrease stitch length.  If long-press, continuously increase or decrease stitch length. |
| Pattern backing-tacking setting |  | If click, set used or cancelled pattern backing-tacking function.  If long-press, switch to pattern backing-tacking mode editing interface. |
| Tight seam setting |  | If click, switch starting tight seam, ending tight seam, full function and function off successively.  If long-press, switch to tight seam mode editing interface. |
| Pattern freedom sewing setting |  | If click, switch to pattern freedom sewing mode selection interface.  If long-press, switch to pattern freedom sewing mode editing interface. |
| Pattern constant-stitch sewing setting |  | If click, switch multi-segment sewing mode or four segments sewing mode.  If long-press, switch to pattern constant-stitch sewing mode editing interface. |
| Start back-tacking sewing |  | If click, switch AB start back-tacking→ABAB start back-tacking→function off→B start back-tacking successively. |
| End back-tacking sewing |  | If click, switch CD end back-tacking→CDCD end back-tacking→function off→C end back-tacking successively. |
| Consecutive reverse sewing |  | If click, set to consecutive reverse sewing mode. |
| Free sewing |  | If click, set to free sewing mode. |
| M key |  | If click, set to multi-segment sewing mode (switch to four-segment sewing, seven-segment sewing, eight-segment sewing, and fifteen-segment sewing in sequence). |
| Auto function |  | 1. If click, set used or cancelled auto function.  2. If long-press, it can restore factory setting. |
| Thread trimming |  | 1. If click, set used or cancelled trimming function.  2. If long-press, enter counter interface. |
| Automatic presser foot lifting setting |  | If click, switch function off→automatic presser foot lifting after trimming→automatic presser foot lifting after pause→full function successively. |
| Half anti-side trample foot lifting |  | If click, set used or cancelled half anti-side trample foot lifting function. |
| Needle stop position selection |  | If click, the needle stop position after shift the sewing mode (upper position / lower position). |
| Slow launch setting |  | 1. If click, set used or cancelled slow launch function.  2. In the parameter setting interface, if long-press, save the current parameter value as factory parameter value. |
| Thread clamping |  | If click, set used or cancelled thread clamping function. |
| Function parameter edit |  | If click, enter or exit the user parameter setting interface.  If long-press, it will switch to the password input interface. Enter the correct password, press S key to confirm, you can enter the advanced parameter setting interface. |
| Setting parameter check and save |  | For the content of the selected parameters check and save: after select parameter press this key to check and modify operation, after modified parameter value press this key to exit and save the parameter.  On the main interface, long press to enter the debugging parameter interface. |
| Parameter increase |  | If click, increase the parameter.  If long-press, continuously increase the parameter. |
| Parameter decrease |  | If click, decrease the parameter.  If long-press, continuously decrease the parameter. |
| Speed increase |  | If click, increase the sewing speed.  If long-press, continuously increase the sewing speed. |
| Speed decrease |  | If click, decrease the sewing speed.  If long-press, continuously decrease the sewing speed. |

**1.2 Auxiliary function**

**1.2.1 Debugging mode**

On the main interface, long-press S key to enter to the debugging parameter interface. P92 correct the electrical angle of motor, P72 upper positioning quick adjustment, P129 back-tacking stepping motor zero-point correction, P74 tacking stitch length compensation and P75 back-tacking stitch length compensation parameter setting.

**1.2.2 Tight seam mode editing**

On the main interface, long-press tight seam key to display "F-1" (starting tight seam), and press the 4th column  ,  to switch between "F-1" (starting tight seam) and "d-2" (ending tight seam), press S to confirm, switch to the editing interface "01 0 0.5", press the 1st or 2nd column  ,  to adjust the number of stitches of 00-12, press the 4th column  ,  to adjust 0 (tacking) -1 (back-tacking). Press  to adjust the stitch length. After the setting is completed, press S key to confirm. Click P key to exit to the main interface.

**1.2.3 Pattern freedom sewing mode**

On the main interface short-press  to shift pattern freedom sewing mode selection interface "n1"， press  to adjust n1-n9.

**1.2.4 Pattern freedom sewing editing**

On the main interface long-press  to shift pattern freedom sewing mode editing interface“n-01 01”，short-press the 4th column  ,  to adjust n01-n09, short-press  adjust 01-10 segment number, adjust to setting pattern number, segment number, short-press S key to confirm, shift to corresponding pattern number editing interface “01 1 3.0”， short press 1st column or 2nd column  ,  to adjust 00-99 stitches, short-press 4th column  ,  1-9 repeat times, short-press  to adjust stitch length, after finished setting short-press S key to confirm. Press P key can exit to interface.

**1.2.5 Pattern back-tacking sewing editing**

On the main interface, long press  to switch the pattern style editing interface "H-01 01", press the 4th column  ,  to adjust the H01-H09 pattern number, and short press  to adjust the 01-10 segment number, segment number, short press S key to confirm, switch to the corresponding pattern number editing interface "01 1 3.0", press the 1st or 2nd column  ,  to adjust the number of 00-99 stitches, press the 4th column  ,  to adjust Repeat 1-9 times, press  to adjust the stitch length. After the setting is completed, press the S key to confirm. Short press P key to exit to the main interface.

**1.2.6 Pattern constant-stitch sewing editing**

In the multi-segment sewing mode, long-press pattern constant-stitch sewing key on the main interface to switch to pattern constant-stitch sewing editing interface "d-01 3.0", press the fourth column  ,  to adjust the d01-d15 segment number, and press  to adjust the current segment stitch length. Short press P key to exit to the main interface.

**2 User parameter**

| No. | Items | Range | Default | Description |
| --- | --- | --- | --- | --- |
| P01 | Free sewing maximum speed (rpm) | 100-4000 | 3700 | Maximum speed of machine sewing. |
| P02 | Set accelerated curve (%) | 10-100 | 80 | Set the acceleration slope.  The greater the slope value, the steeper the speed; the smaller the slope value, the slower the speed. |
| P03 | Needle UP/ DOWN | UP/DN | DN | UP: Upper needle stop position  DN: Lower needle stop position |
| P04 | Start back-tacking speed (rpm) | 200-3200 | 2000 |  |
| P05 | End back-tacking speed (rpm) | 200-3200 | 2000 |  |
| P06 | Bar-tacking speed (rpm) | 200-3200 | 2000 |  |
| P07 | Soft start speed after second stitch (rpm) | 200-1500 | 1500 |  |
| P08 | Stitch numbers for soft start | 1-15 | 2 |  |
| P09 | Automatic constant-stitch sewing speed (rpm) | 200-4000 | 3700 | Speed adjustment for automatic constant-stitch sewing. |
| P10 | Automatic end back-tacking sewing after constant-stitch sewing | ON/OFF | ON | ON: After executing the constant-stitch sewing, the back-tacking sewing will be executed automatically. In any sewing mode, mending stitch function cannot be used.  OFF: After executing the last constant-stitch sewing, the back-tacking sewing function will not be automatically executed, and the front step or full back step must be performed again. |
| P11 | Back-tacking stitch overall compensation | -20~20 | 10 |  |
| P12 | Start back-tacking running mode selection | 0-1 | 1 | 0: Controlled by foot pedal, can be stopped and started at will.  1: Touch the foot pedal to automatically execute back-tacking action. |
| P13 | Ending mode of start  back-tacking | CON/STP | CON | CON: Start back-tacking is completed automatically continued for next action.  STP: After the number of stitches is completed, stop automatically. |
| P14 | Slow start function selection | ON/OFF | OFF |  |
| P15 | Manual Switch A | 0-6 | 5 | 0: OFF  1: Half stitch  2: One stitch  3: Continuous half stitch  4: Continuous one stitch  5: Back-tacking when machine stop or pause  6: Tight seam function (press and hold the key to sew) |
| P16 | Speed limit of manual back-tacking | 0-3200 | 0 | The function is disabled when the value is less than 100. |
| P17-N04 | Language setting | 0-9 | 1 | 0: OFF  1: Chinese  2: English  3: Vietnamese  4: Portuguese  5: Turkish  6: Spanish  7: Russian  8: Arabic |
| P17-N05 | Voice broadcast selection | 0-3 | 1 | 0: No key tone, no error voice  1: With key tone and error voice  2: Key tone only  3: Error voice only |
| P17-N06 | Automatic piece counting function | 0-50 | 1 | 0: OFF  1-50: Trimming counting times setting |
| P17-N08 | Virtual and real speed function switch | 0-1 | 0 | For each increase of 100 above 4000 rpm, the actual increase is 100\*[P17-N09]. |
| P17-N09 | Virtual and real speed ratio (%) | 10-100 | 50 |  |
| P17-N12 | Boot counter interface selection | 0-1 | 0 | 0: OFF  1: ON |
| P17-N13 | Automatic piece counting mode selection | 0-1 | 0 | 0: Incremental piecework mode  1: Diminishing piecework mode |
| P18 | Start back-tacking compensation 1 | 0-200 | 136 | Stitch compensation for start back-tacking A section, 0~200 action gradually delay; The large value, the longer of the A section last stitch, and the shorter of the B section first stitch. |
| P19 | Start back-tacking compensation 2 | 0-200 | 134 | Stitch compensation for start back-tacking A section, 0~200 action gradually delay; The large value, the longer of the B section last stitch. |
| P20 | End back-tacking running mode selection | 0-1 | 1 |  |
| P21 | The position of the pedal for accelerating | 30-1000 | 520 |  |
| P22 | The position of the pedal for the stop | 30-1000 | 420 |  |
| P23 | The position of the pedal for presser foot lifting | 30-1000 | 270 |  |
| P24 | The position of the pedal for thread trimming | 30-500 | 130 |  |
| P25 | End back-tacking compensation 3 | 0-200 | 136 | Stitch compensation for end back-tacking C section, 0~200 action gradually delay; The large value, the shorter of the C section first stitch. |
| P26 | End back-tacking compensation 4 | 0-200 | 140 | Stitch compensation for end back-tacking D section,0~200 action gradually delay; the large value, the longer of the C section last stitch, and the shorter of the D section first stitch. |
| P28 | Bar-tacking running mode  selection | 0-1 | 1 |  |
| P29 | The strength of thread trimming stop | 1-45 | 20 |  |
| P30 | The foot lift height of thread tension release start action when knee-control foot lift | 0-4799 | 3200 |  |
| P31 | Thread tension release function switch when knee-control foot lift | 0-1 | 1 |  |
| P32 | Bar-tacking compensation 5 | 0-200 | 140 | Stitch compensation for bar-tacking A (C) section, 0~200 action gradually delay; the large value, the longer of the A (C) section last stitch; the shorter of the B (D) section first stitch. |
| P33 | Bar-tacking compensation 6 | 0-200 | 136 | Stitch compensation for bar-tacking B (D) section, 0~200 action gradually delay; the large value, the longer of the B (D) section last stitch; the shorter of the C section first stitch. |
| P34 | Constant-stitch sewing running mode selection | A/M | A | A: Touch the foot pedal to automatically execute constant-stitch sewing action  M: Controlled by foot pedal, can be stopped and started at will |
| P35 | Thread tension releasing function setting when presser foot lifting action | 0-2 | 1 | 0: OFF  1: Thread tension releasing output function ON when presser foot lifting, thread tension releasing output function OFF when stopover  2: Full function |
| P36 | Thread tension releasing function selection | 0-1 | 1 | 0: OFF  1: ON |
| P37 | Thread wiping function / Thread clamping function selection | 0-11 | 8 | 0 : OFF  1: Thread wiping function  2-11: Thread clamping Function and the strength of automatic thread clamping. |
| P38 | Automatic thread trimming function selection | ON/OFF | ON |  |
| P39 | [Automatic presser foot lifting](C:/Users/Administrator/AppData/Local/youdao/dict/Application/7.2.0.0703/resultui/dict/javascript:;) when pause function selection | UP/DN | DN |  |
| P40 | [Automatic presser foot lifting](C:/Users/Administrator/AppData/Local/youdao/dict/Application/7.2.0.0703/resultui/dict/javascript:;) after trimming function selection | UP/DN | DN |  |
| P41 | Thread trimming counter display | 0-9999 | 0 | Display the quantity of finished sewing piece. Long-press “-” key to clear the count. |
| P42-N01 | The control system version number |  |  |  |
| P42-N02 | The panel version number |  |  |  |
| P42-N03 | Speed |  |  |  |
| P42-N04 | The pedal AD |  |  |  |
| P42-N05 | The mechanical angle(upper position) |  |  |  |
| P42-N07 | Bus bar voltage AD |  |  |  |
| P42-N12 | Knee-control position sensor AD value |  |  |  |
| P42-N14 | The control system version number 2 |  |  |  |
| P42-N15 | Stepping drive version number |  |  |  |
| P42-N16 | Stitch counter display (every 10 stitches, the value changes by 1) |  |  |  |
| P42-N17 | Number of needles for maintenance operation (10,000 needles) \*10 |  |  |  |
| P42-N18 | Simulating action of thread trimming |  |  |  |
| P42-N19 | Electronic wrench AD value |  |  |  |
| P42-N21 | Thread trimming origin debugging |  |  |  |
| P42-N22 | Presser foot origin debugging |  |  |  |
| P43 | Motor rotation direction setting | CCW/CW | CCW | CW: Clockwise  CCW: Counter clock wise |
| P44 | Brake strength during stopover | 1-45 | 16 |  |
| P45 | Pattern freedom sewing mode selection | 0-1 | 0 | 0: Controlled by foot pedal, can be stopped and started at will  1: Touch the foot pedal to automatically execute a pattern sewing action |
| P46 | Motor stop with a reverse angle after trimming function | ON/OFF | OFF |  |
| P47 | Adjust the reverse angle when motor stop after trimming | 10-300 | 40 | Start from the upper needle position and adjust the angle of the needle lift in reverse operation after trimming. |
| P48 | The minimum speed (positioning speed) (rpm ) | 100-500 | 210 | Adjust the minimum speed |
| P49 | Thread trimming speed (rpm) | 100-500 | 300 | Adjust thread trimming speed |
| P52 | Delay the start of the motor to protect the lowering time of presser foot (ms) | 10-990 | 120 | Delay the start time, with automatic presser foot down. |
| P53 | Half back pedaling lifting presser foot function to cancel | 0-2 | 1 | 0: OFF  1: Back pedaling and half back pedaling with lifting presser foot  2: Half back pedaling without lifting presser foot, back pedaling with lifting presser foot |
| P54 | Thread trimming action time (ms) | 10-990 | 60 |  |
| P55 | Thread wiping action time (ms) | 10-990 | 30 |  |
| P56 | Power on and positioning | 0-1 | 0 | 0: Always do not find the upper positioning  1: Always find the upper positioning |
| P57 | Presser foot solenoid protection time (s) | 1-60 | 5 | Forced shutdown after hold time to prevent the electromagnet from being hot for a long time |
| P58 | Upper positioning adjustment | 0-359 |  | Upper positioning adjustment, the needle will advance stop when the value decreased, the needle will delay stop when the value increased. |
| P59 | Lower positioning adjustment | 0-359 |  | Lower positioning adjustment, the needle will advance stop when the value decreased, the needle will delay stop when the value increased. |
| P60 | Testing speed (rpm ) | 100-4000 | 3500 | Setting testing speed. |
| P61 | Testing A | ON/OFF | OFF | Continuous running testing. |
| P62 | Testing B | ON/OFF | OFF | Start and stop testing with all functions. |
| P63 | Testing C | ON/OFF | OFF | Start and stop testing without all function. |
| P64 | Test run time | 1-250 | 30 |  |
| P65 | Test stop time | 1-250 | 10 |  |
| P66 | Machine protection switch selection | 0-1 | 1 | 0: Disable  1: Testing zero signal |
| P67 | Electronic wrench function selection | ON/OFF | ON |  |
| P69 | Pattern freedom sewing speed | 100-3000 | 2000 |  |
| P70 | Model selection |  | 28 |  |
| P71 | Correction stitches distance of manual button A | 0-5.0 | 0 |  |
| P72 | Upper positioning quick adjustment | 0-359 |  | Adjust upper needle stop position, the displayed value will change with the position of the handwheel, press "S" key to save the current position (value) as up needle position. |
| P73 | Lower positioning quick adjustment | 0-359 |  | Adjust lower needle stop position, the displayed value will change with the position of the handwheel, press "S" key to save the current position (value) as down needle position. |
| P74 | Tacking stitch length compensation | -100~100 | 0 |  |
| P75 | Back-tacking stitch length compensation | -100~100 | 0 |  |
| P76 | The working time of the full output of thread clamping (ms) | 0-5 | 0 |  |
| P77 | Opportunity point of back-tacking for end back-tacking in high speed in free sewing mode | 0-350 | 130 |  |
| P78 | The start angle of thread clamping | 5-359 | 100 |  |
| P79 | The stop angle of thread clamping | 5-359 | 270 |  |
| P80 | The main shaft angle when first engage start (start of the split line) (define down position as 0 point) | 0-359 | 65 |  |
| P81 | The main shaft angle when first engage end (end of the split line) (define down position as 0 point) | 0-359 | 140 |  |
| P82 | The main shaft angle when second engage start (define down position as 0 point) | 0-359 | 170 |  |
| P83 | Stopping strength after trimming | 10-100 | 20 |  |
| P86 | Upper and lower positioning distance | 15-345 | 180 | Upper and lower positioning distance angle (1 degree for every 4 values). |
| P87 | Wiping thread return delay time | 10-990 | 50 | Make sure the wiper returns to its original position. |
| P88 | Stopover distance | 10-100 | 30 |  |
| P89 | AC overvoltage setting | 500-1023 | 880 |  |
| P90 | Soft start first stitch speed | 200-1500 | 400 |  |
| P91 | Soft start second stitch speed | 200-1500 | 1000 |  |
| P92 | Correct the electrical angle of motor |  |  | Reading the initial Angle of encoder, the factory default was set, please do not change the values (parameter value cannot be changed manually, random change it will result the control box and motor abnormal or damaged). |
| P93 | The starting time of the half back pedaling function (ms) | 10-900 | 100 |  |
| P98 | Thread tension releasing protection time (s) | 0-10 | 2 |  |
| P99 | Starting tight seam stitch length | 0-5.0 | 0.5 |  |
| P100 | Direction of starting tight seam | 0-1 | 0 |  |
| P101 | The start angle of thread tension releasing | 1-359 | 30 | Thread tension releasing start angle (defined as 0°under calculation). |
| P102 | The stop angle of thread tension releasing | 1-359 | 180 | Thread tension releasing end angle (defined as 0°under calculation, must be greater than P101 parameter value). |
| P103 | Periodic signal of thread tension releasing output (%) | 1-8 | 3 |  |
| P104 | Pause time when constant-stitch sewing switch to end back-tacking sewing | 0-990 | 100 |  |
| P105 | Pattern freedom sewing mode selection | 0-9 | 0 | 0: OFF  1-9: Pattern freedom sewing mode |
| P107 | Starting tight seam speed | 100-2000 | 1000 |  |
| P108 | Starting tight seam stitch number | 0-12 | 1 |  |
| P109 | The delay time before thread  wiping | 5-990 | 220 | Interval time before entering thread wiping action after finding the upper positioning. |
| P110 | Trimming back time (ms) | 60-990 | 100 | Make sure the thread trimming device returns to its original position. |
| P111 | Clamp function without any thrum switch | 0-1 | 0 |  |
| P112 | The delay time before thread hooking with clamp function without any thrum | 0-990 | 90 |  |
| P113 | The thread hooking action time with clamp function without any thrum | 0-990 | 90 |  |
| P114 | The return back time of thread hooking with clamp function without any thrum | 0-990 | 30 |  |
| P115 | Duty cycle for thread hooking with clamp function without any thrum | 0-100 | 80 |  |
| P116 | The suction time for clamp function without any thrum | 0-5000 | 700 |  |
| P117 | Duty cycle for thread pushing with clamp function without any thrum | 0-100 | 80 |  |
| P118 | Function selection of manual back-tacking button in pattern mode | 0-1 | 1 |  |
| P119 | Electromagnet overcurrent protection detection switch | 0-1 | 0 |  |
| P120 | Oil level detection switch | 0-1 | 0 |  |
| P122 | Kneeling device starting AD value | 0-1023 | 600 |  |
| P125 | The height of the presser foot lifting in the middle | 3050-3800 | 3600 |  |
| P126 | The highest presser foot lift height of electric knee-control | 1000-1100 | 1050 |  |
| P127 | Knee-control function selection | 0-2 | 1 | 0: OFF  1: Valid when the main shaft motor is stopped  2: Valid when the main shaft motor is running and stopped |
| P129 | Stepping motor zero-point of stitch length correction | -500~500 | 0 |  |
| P131 | Normal stitch length | 0-5.0 | 5.0 |  |
| P132 | Manual close stitches distance | 0-5.0 | 2.0 |  |
| P133 | Electronic wrench start AD value | 0-1023 | 400 |  |
| P134 | Electronic wrench end AD value | 0-1023 | 60 |  |
| P135 | The lowest presser foot lift height of electric knee-control | 0-4799 | 4100 |  |
| P136 | The highest of presses foot lift highness | 3050-3150 | 3100 |  |
| P137 | Stepping stroke of the first engage | 0-4799 | 1150 |  |
| P138 | The maximum limit stepping speed of the first engage | 50-800 | 380 |  |
| P139 | Stepping stroke of the second engage | 0-4799 | 1600 |  |
| P140 | The maximum limit stepping speed of the second engage | 50-800 | 150 |  |
| P143 | Tight seam mode selection | 0-3 | 0 | 0: OFF  1: Starting tight seam  2: Ending tight seam  3: Full function |
| P144 | Tacking stitch length compensation in high speed | -100~100 | 15 |  |
| P145 | Back-tacking stitch length compensation in high speed | -100~100 | 15 |  |
| P146 | Presser foot speed | 50-800 | 150 |  |
| P148 | When sewing, the highest presser foot lift height of electric knee-control | 0-4799 | 50 |  |
| P153 | Ending tight seam stitch length |  | 5 |  |
| P154 | Ending tight seam speed | 100-2000 | 1000 |  |
| P155 | Manual stitching button function switch | 0-1 | 0 | 0: Darning stitch  1: Tight seam |
| P159 | Direction of ending tight seam | 0-1 | 0 | 0: Forward  1: Backward |
| P160 | Ending tight seam stitch number | 0-12 | 1 |  |
| P165 | Stitch counter mode selection | 0-4 | 0 | 0: Do not count  1: Increase cycle count  2: Decrease cycle count  3: Increase count, alarm after the count is full, need to press the clear key to start recounting  4: Decrease count, alarm after the count is full, need to press the clear key to start recounting |
| P166 | Upper limit of stitch counter (stitch) \*10 | 0-9999 | 500 |  |
| P167 | Upper limit of maintenance stitch number (10000 stitch) \*10 | 0-9999 | 0 |  |
| P168 | Main shaft motor type selection | 0-9999 | 6 |  |
| P170 | Correction stitches distance of manual button B | 0-5.0 | 0 |  |
| P171 | Correction stitches distance of manual button C | 0-5.0 | 2.0 |  |
| P172 | The highest of presser foot lift highness limit | 0-4799 | 4799 |  |
| P173 | Correction stitches distance of manual button D | 0-5.0 | 1.0 |  |
| P174 | Manual Switch B | 0-6 | 3 | 0: OFF  1: Half stitch  2: One stitch  3: Continuous half stitch  4: Continuous one stitch  5: Back-tacking when machine stop or pause  6: Tight seam function |
| P175 | Manual Switch C | 0-6 | 3 | 0: OFF  1: Half stitch  2: One stitch  3: Continuous half stitch  4: Continuous one stitch  5: Back-tacking when machine stop or pause  6: Tight seam function |
| P176 | Manual Switch D | 0-6 | 3 | 0: OFF  1: Half stitch  2: One stitch  3: Continuous half stitch  4: Continuous one stitch  5: Back-tacking when machine stop or pause  6: Tight seam function |
| P177 | 1mm forward stitch length reference value setting | 0-2000 | 70 |  |
| P178 | 1mm backward stitch length reference value setting | 0-2000 | 70 |  |
| P179 | 2mm forward stitch length reference value setting | 0-2000 | 140 |  |
| P180 | 2mm backward stitch length reference value setting | 0-2000 | 140 |  |
| P181 | 3mm forward stitch length reference value setting | 0-2000 | 210 |  |
| P182 | 3mm backward stitch length reference value setting | 0-2000 | 210 |  |
| P183 | 4mm forward stitch length reference value setting | 0-2000 | 285 |  |
| P184 | 4mm backward stitch length reference value setting | 0-2000 | 280 |  |
| P185 | 5mm forward stitch length reference value setting | 0-2000 | 380 |  |
| P186 | 5mm backward stitch length reference value setting | 0-2000 | 375 |  |
| P187 | 6mm forward stitch length reference value setting | 0-2000 | 500 |  |
| P188 | 6mm backward stitch length reference value setting | 0-2000 | 495 |  |
| P189 | 7mm forward stitch length reference value setting | 0-2000 | 540 |  |
| P190 | 7mm backward stitch length reference value setting | 0-2000 | 575 |  |
| P205 | The speed of the first stitch at the start of sewing (rpm) | 0-2000 | 0 |  |
| P206 | The speed of the second stitch at the start of sewing (rpm) | 0-2000 | 0 |  |
| P207 | The speed of the third stitch at the start of sewing (rpm) | 0-4000 | 0 |  |
| P211 | Periodic signal of the first thread tension release output action (%) | 1-100 | 50 |  |
| P212 | Thread tension release the first output action time | 1-100 | 20 |  |
| P221 | Pedal top speed position | 30-1000 | 890 |  |
| P222 | Pedal gear switch | 0-1 | 0 | 0: Normal gear  1: High speed gear |
| P226 | The main shaft angle when returning to normal stitch length when starting a stitch or cranking the handwheel by hand | 0-359 | 80 |  |
| P227 | Stepping first stroke when zero point of the presser foot return to the normal stitch length | 0-4799 | 80 |  |
| P228 | Stepping first speed when zero point of the presser foot return to the normal stitch length | 50-1000 | 800 |  |
| P229 | Stepping second speed when zero point of the presser foot return to the normal stitch length | 10-1000 | 500 |  |
| P230 | The switch of each constant-stitch sewing with start back-tacking sewing, end back-tacking sewing and trimming | 0-1 | 0 | 0: OFF  1: ON |
| P231 | Stepping first stroke when zero point of the trimming return to the normal stitch length | -50~50 | -40 |  |
| P232 | Stepping first speed when zero point of the trimming return to the normal stitch length | 0-9999 | 0 |  |
| P233 | Stepping second speed when zero point of the trimming return to the normal stitch length | 0-9999 | 0 |  |
| P234 | Mode selection when pause in pattern sewing | 0-1 | 0 |  |
| P235 | Pattern sewing compensation 1 | 0-200 | 136 |  |
| P236 | Pattern sewing compensation 2 | 0-200 | 132 |  |
| P237 | Start back-tacking stitch compensation 11 | 0-200 | 138 |  |
| P238 | Start back-tacking stitch compensation 12 | 0-200 | 138 |  |
| P239 | End back-tacking stitch compensation 13 | 0-200 | 138 |  |
| P240 | End back-tacking stitch compensation 14 | 0-200 | 138 |  |
| P241 | Back-tacking stitch compensation 15 | 0-200 | 138 |  |
| P242 | Back-tacking stitch compensation 16 | 0-200 | 136 |  |
| P251 | The speed of returning to the stepping motor zero-point position of stitch length after thread trimming | 0-1000 | 320 |  |
| P252 | Stepping motor zero-point position of the thread trimming adjustment | 0-4799 | 600 |  |
| P253 | Stepping motor zero-point position of the presser foot adjustment | 0-4799 | 500 |  |
| P254 | 7mm tacking stitch length compensation in high speed | -100~100 | 0 |  |
| P255 | 7mm back-tacking stitch length compensation in high speed | -100~100 | 0 |  |

Note: the initial value of parameters is for reference only, and the actual value of parameters is subject to the real object.

**3 Error code list**

|  |  |  |
| --- | --- | --- |
| Error Code | Problem description | Solutions |
| E01 | High voltage | 1. Whether the grid voltage is higher than AC260V.  2. If it is self-generated power supply, please reduce the generator power.  3. If it still does not work normally, please replace the control box and notify the after-sales service. |
| E02 | Low voltage | 1. Whether to connect to low voltage.  2. Reset.  3. If it still does not work normally, please replace the control box and notify the after-sales service. |
| E03 | CPU communication abnormal | 1. Turn off the system power and check whether the connection of the display screen is loose or disconnected, restart the system after returning it to normal.  2. Turn off the system power, remove the control box and only plug in the power cord to power on, whether alarm E05, if it still alarms E03, replace the control box and notify the after-sales service. |
| E05 | Pedal signal abnormal | 1. Check whether the pedal connector is loose or fall off, and restart the system after returning it to normal.  2. If it still does not work normally, please replace the control box or speed controller and notify the after-sales service. |
| E07 | Main shaft motor locked-rotor | 1. Turn off the power and check whether the handwheel can be turned smoothly (turn the handwheel by hand), if it cannot be turned, please check the machine;  2. Turn off the power, check whether the motor power connector is loose, plug it in and restart it;  3. Check whether the upper needle stop position is correct, if not, please adjust the upper positioning position;  4. If it still does not work normally, please replace the control box or spindle motor and notify the after-sales service. |
| E10 | Electromagnet overcurrent | 1. Unplug the solenoid connector, if alarm E10, replace the control box and notify the after-sales service.  2. If there is no alarm after removing the solenoid connector, please plug it back in  1) Step on the front pedal to let the sewing machine perform thread clamping and back-tacking. If alarms, please turn off start back-tacking and end back-tacking, restart the control box, and then step forward. If alarms, please turn off the thread clamping function and restart the electronic control, and step forward again. If there is no alarm, replace the clamper.  2) Step on the front pedal to let the sewing machine perform thread clamping, back-tacking and half anti-side trample foot lifting. If there is no alarm, please back pedaling thread trimming, if it alarms, please replace thread tension releasing solenoid. |
| E09  E11 | The positioning signal of main shaft motor encoder is abnormal | 1. Turn off the system power, check whether main shaft motor encoder connector is loose or fall off, restore it to normal and restart the system.  2. Check whether the motor zero point correction setting is correct; Reset the motor zero point correction; Whether there is oil on the encoder code plate, please clean it if there is any;  3. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service. |
| E14 | Main shaft motor encoder signal is abnormal | 1. Turn off the system power, check whether the main shaft motor encoder connector is loose or fall off, restore it to normal and restart the system.  2. Check whether the grating is installed correctly (whether the grating screws are tightened and whether the grating is in the center of the encoder).  3. Check whether there is oil on the encoder code plate, if there is, please clean it up, and restart the system after recovery.  4. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service. |
| E15 | Main shaft motor drive overcurrent | 1. Please check whether the motor power cord has bad contact.  2. Please check whether the motor power cord is crushed.  3. Please replace the control box or main shaft motor and notify the after-sales service. |
| E17 | Machine overturned | 1. Turn off the system power and check if the machine is overturned.  2. Check whether the machine protection switch detection setting is correct.  3. If it still does not work normally, please replace the control box or panel and notify the after-sales service. |
| E20 | Main shaft motor failed to start | 1. Turn off the system power, check whether main shaft motor power cord connector and encoder connector are loose or fall off, restore them to normal and restart the system.  2. Check whether the motor zero point correction setting is correct, reset the motor zero point correction  3. If it still does not work normally, please replace the control box or main shaft motor and notify the after-sales service. |
| E28 | Maintenance warning | Please perform maintenance. (When an alarm occurs, press the S key to clear and re-count.) |
| E51 | Insufficient bobbin thread warning | Please add bobbin thread. |
| E80 | Abnormal communication between main chip and drive chip | Please replace the control box and notify the after-sales service. |
| E82 | Back-tacking stepping motor  overcurrent | 1. Turn off the system power and observe whether back-tacking stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether connector of back-tacking stepping motor is loose or fall off, restore it to normal and restart the system.  2. If it still does not work normally, please replace the control box or back-tacking stepping motor and notify the after-sales service. |
| E84 | The positioning signal of back-tacking stepping motor encoder is abnormal | 1. Turn off the system power and observe whether back-tacking stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether the encoder connector of back-tacking stepping motor is loose or fall off, and restart the system after returning it to normal.  2. Check whether the grating is installed correctly (whether the grating screws are fastened and whether the grating is in the center of the encoder);  3. Check if there is oil on the grating code plate, if so, please clean it up, and restart the system after restoration;  4. If it still does not work normally, please replace the control box or back-tacking stepping motor and notify the after-sales service. |
| E85 | Back-tacking motor encoder signal is abnormal | 1. Turn off the power of the system, check whether the encoder connector of back-tacking stepping motor is loose or fall off, restore it to normal and restart the system.  2. Check whether the grating is installed correctly (whether the grating screws are fastened and whether the grating is in the center of the encoder);  3. Check if there is oil on the grating code plate, if so, please clean it up, and restart the system after restoration;  4. If it still does not work normally, please replace the control box or back-tacking stepping motor and notify the after-sales service. |
| E86 | Back-tacking stepping motor failed to start | 1. Turn off the power of the system, check whether the power cord connector of back-tacking stepping motor and the encoder connector are loose or fall off, restore them to normal and restart the system.  2. Check whether the grating is installed correctly (whether the grating screws are fastened and whether the grating is in the center of the encoder);  3. Check if there is oil on the grating code plate, if so, please clean it up, and restart the system after restoration;  4. If it still does not work normally, please replace the control box or back-tacking stepping motor and notify the after-sales service. |
| E87 | Back-tacking stepping motor locked-rotor | 1. Turn off the system power and observe whether back-tacking stepping motor is stuck. If it is stuck, remove the mechanical failure of the machine first. If it is normal, check whether the power cord connector of back-tacking motor and the encoder connector are loose or fall off, restore them to normal and restart the system.  2. If it still does not work normally, please replace the control box or back-tacking stepping motor and notify the after-sales service. |

**4 Port diagram**

**8P function port description**



1. Suction with clamp function without any thrum: 1, 5

2. Thread hooking with clamp function without any thrum: 2, 6

3. Thread clamping (thread wiping) / Thread pushing with clamp function without any thrum: 3, 7 (+32V)

4. Thread tension releasing: 4, 8 (+32V)

**10P (small) function port description**



1. 1/2 manual darning stitch signal: 8

2. 1/4 manual darning stitch signal: 3

3. Manual back-tacking signal: 4

4. Manual darning stitch signal: 5

5. LED Light: 9 (+5V), 10 (DGND)